Those are the right ones, you'd need two of the 13943-2H for the rear. On the front you need 1 13943-2, and 1 13943-8. They are a medium weight, we no longer give durometer ratings to the elastomers.